
Step1: Select DIO virtual COM port then connect it.



Step2: Click “Start” to upgrade the new firmware.

